<?xml version="1.0"?>
<!--
FILE INFORMATION

OMA Permanent Document
   File: OMA-SUP-RDF_ccppschema_mms-V1_3-20110511-C.txt
   Type: Text

Public Reachable Information
   Path: http://www.openmobilealliance.org/tech/profiles/MMS
   Name: ccppschema_mms-v1_3

NORMATIVE INFORMATION

Information about this file can be found in the MMS 1.3 Enabler Release available at
http://www.openmobilealliance.org/

Send comments to technical-comments@mail.openmobilealliance.org
	
LEGAL DISCLAIMER

  Use of this document is subject to all of the terms and conditions
  of the Use Agreement located at
  http://www.openmobilealliance.org/UseAgreement.html,
  provided, however, that section (d) under "Documents - Terms 
  of Use" which states, "no modifications are made to such 
  Documents" does not apply to your use.

  The Open Mobile Alliance authorizes you to copy this document, 
  provided that you retain all copyright and other proprietary  
  notices contained in the original materials on any copies of the 
  materials and  that you comply strictly with these terms. This 
  copyright permission does not constitute an endorsement of the 
  products or services. The Open Mobile Alliance assumes no 
  responsibility for errors or omissions in this document.


  Each Open Mobile Alliance member has agreed to use reasonable
  endeavors to inform the Open Mobile Alliance in a timely manner of
  Essential IPR as it becomes aware that the Essential IPR is related
  to the prepared or published specification.  However, the members
  do not have an obligation to conduct IPR searches.  The declared
  Essential IPR is publicly available to members and non-members of
  the Open Mobile Alliance and may be found on the "OMA IPR
  Declarations" list at http://www.openmobilealliance.org/ipr.html.
  The Open Mobile Alliance has not conducted an independent IPR review
  of this document and the information contained herein, and makes no
  representations or warranties regarding third party IPR, including
  without limitation patents, copyrights or trade secret rights.  This
  document may contain inventions for which you must obtain licenses
  from third parties before making, using or selling the inventions.
  Defined terms above are set forth in the schedule to the Open Mobile
  Alliance Application Form.

  NO REPRESENTATIONS OR WARRANTIES (WHETHER EXPRESS OR IMPLIED) ARE
  MADE BY THE OPEN MOBILE ALLIANCE OR ANY OPEN MOBILE ALLIANCE MEMBER
  OR ITS AFFILIATES REGARDING ANY OF THE IPR'S REPRESENTED ON THE "OMA
  IPR DECLARATIONS" LIST, INCLUDING, BUT NOT LIMITED TO THE ACCURACY,
  COMPLETENESS, VALIDITY OR RELEVANCE OF THE INFORMATION OR WHETHER OR
  NOT SUCH RIGHTS ARE ESSENTIAL OR NON-ESSENTIAL.

  THE OPEN MOBILE ALLIANCE IS NOT LIABLE FOR AND HEREBY DISCLAIMS ANY
  DIRECT, INDIRECT, PUNITIVE, SPECIAL, INCIDENTAL, CONSEQUENTIAL, OR
  EXEMPLARY DAMAGES ARISING OUT OF OR IN CONNECTION WITH THE USE OF
  DOCUMENTS AND THE INFORMATION CONTAINED IN THE DOCUMENTS.

  Copyright 2011 Open Mobile Alliance Ltd.  All Rights Reserved.
  Used with the permission of the Open Mobile Alliance Ltd. under the
  terms set forth above.

-->

<!DOCTYPE rdf:RDF [
  <!ENTITY ns-rdf  'http://www.w3.org/1999/02/22-rdf-syntax-ns#'>
  <!ENTITY ns-rdfs 'http://www.w3.org/2000/01/rdf-schema#'>
  <!ENTITY ns-prf  'http://www.openmobilealliance.org/tech/profiles/MMS/ccppschema_mms-v1_3'>
  <!ENTITY ns-prf-base 'http://www.openmobilealliance.org/tech/profiles/UAPROF/ccppschema-20030226#'>
  <!ENTITY prf-dt  'http://www.openmobilealliance.org/tech/profiles/UAPROF/xmlschema-20030226#'>
  <!ENTITY xsd     'http://www.w3.org/2001/XMLSchema#'>
]>

<rdf:RDF
  xmlns      = '&ns-rdf;'
  xmlns:rdf  = '&ns-rdf;'
  xmlns:rdfs = '&ns-rdfs;'
  xmlns:prf  = '&ns-prf;'
  xmlns:prf-base ='&ns-prf-base;'>


<!-- ****************************************************************** -->
<!-- ***** Component Definitions ***** -->

<rdf:Description rdf:ID="MmsCharacteristics">
  <rdf:type rdf:resource="&ns-rdf;Class"/>
  <rdfs:subClassOf rdf:resource="&ns-rdfs;Component"/>
  <rdfs:label xml:lang='en'>Component: MmsCharacteristics</rdfs:label>
  <rdfs:comment xml:lang='en'>
  The MmsCharacteristics component contains properties of the device's
  Multimedia messaging capabilities, such as maximum message size, maximum
  image resolution, etc.
  </rdfs:comment>
</rdf:Description>


<!-- ****************************************************************** -->
<!-- ***** Component: MmsCharacteristics ***** -->
<!-- ****************************************************************** -->
<!-- ***** Attributes for component:   MmsCharacteristics ***** -->

<rdf:Description rdf:ID="MmsMaxMessageSize">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: Maximum size of an MMS message in bytes.
   Examples:   	2048 
   </rdfs:comment>
   <rdfs:range rdf:resource='&prf-dt;Number'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>


<rdf:Description rdf:ID="MmsMaxImageResolution">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: The maximum size of an image in units of pixels 
   (horizontal x vertical).
   Examples:   	80x60
   </rdfs:comment>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>



<rdf:Description rdf:ID="MmsCcppAccept">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: Property value is a list of supported content types
   where each item in the list is a content type name
   registered as a MIME type
   Examples:   	“image/jpeg? “audio/wav? “video/mpeg-4?
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>


<rdf:Description rdf:ID="MmsCcppAcceptCharSet">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: List of character sets that the MMS Client supports.
   Property value is a list of character sets, where 
   each item in the list is a character set name registered
   with IANA
   Examples:   	“US-ASCII? “ISO-8859-1?
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsCcppAcceptLanguage">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: List of preferred languages. The first item in the
   list should be considered the user’s first choice. 
   Property value is a list of natural languages, where
   each item in the list is the name of a language as 
   defined by RFC 1766.
   Examples:   	“en? “fr?
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsCcppAcceptEncoding">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: List of transfer encodings that the MMS Client supports.
   Property value is a list of transfer encodings, where 
   each item in the list is a transfer encoding name as 
   specified by RFC 2045 and registered with IANA.
   Examples:   	“base64? “quoted-printable"
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsVersion">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: The MMS versions supported by the MMS Client conveyed 
   as majorVersionNumber.minorVersionNumber.
   Examples:   	"2.0", "1.3"
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsCcppStreamingCapable">
   <rdf:type rdf:resource="&ns-rdf;Property"/> 
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: Indicates whether the MMS Client is capable of invoking     
   streaming.
   Examples:   	"Yes", "No"
   </rdfs:comment>
   <rdfs:range rdf:resource='&prf-dt;Boolean'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsSmilBaseSet">
  <rdf:type rdf:resource="&ns-rdf;Property"/>
  <rdfs:domain rdf:resource="#MmsCharacteristics"/>
  <rdfs:comment xml:lang='en'>
  Description: Indicates one or more base sets of SMIL modules that the
  client supports. Legal values are the following pre-defined
  identifiers: "SMIL-CONF-1-2" indicates the SMIL base set and 
  associated limitations defined in the OMA MMS Conformance Document. Values defined in 
  3GPP TS 26.234 for the "SmilBaseSet" component may also be used.
  Examples: "SMIL-CONF-1-2", "SMIL-3GPP-R4", "SMIL-3GPP-R5"
  </rdfs:comment>
  <rdfs:range rdf:resource="&ns-rdf;Bag"/>
  <rdfs:range rdf:resource='&prf-dt;Literal'/>
  <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsContentClass">
   <rdf:type rdf:resource="&ns-rdf;Property"/>
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: Property value is a list of supported content            
   classes where each item in the list is an MM content class as defined in the MMS Conformance Document.
   Examples:   	“TX? “IB? “IR? “VB? “VR?
   </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsSuppressContentAdaptation">
  <rdf:type rdf:resource="&ns-rdf;Property"/>
  <rdfs:domain rdf:resource="#MmsCharacteristics"/>
  <rdfs:comment xml:lang='en'>
  Description: Indicates that no content adaptation is to be performed by the MMS Proxy-Relay.
  Examples: "Yes", "No"
  Default: "No"
  </rdfs:comment>
  <rdfs:range rdf:resource='&prf-dt;Boolean'/>
  <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsXHTMLBaseSet">
  <rdf:type rdf:resource="&ns-rdf;Property"/>
  <rdfs:domain rdf:resource="#MmsCharacteristics"/>
  <rdfs:comment xml:lang='en'>
    Description: Indicates one or more base sets of XHTML that the
    client supports in SMIL text regions in the context of retrieval/presentation. Legal
    values are the following pre-defined identifiers: "XHTMLMP-CONF-1-3" indicates the XHTML
    MP base set and associated limitations defined in the OMA MMS Conformance Document for
    retrieval and presentation.

    Type: Literal bag
    Resolution: Locked
    Examples: " XHTMLMP-CONF-1-3", "XHTMLMP-FULL-1-0", "XHTMLMP-FULL-1-1"
  </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsApplicAddressingCapable">
   <rdf:type rdf:resource="&ns-rdf;Property"/> 
   <rdfs:domain rdf:resource="#MmsCharacteristics"/>
   <rdfs:comment xml:lang='en'>
   Description: Indicates whether the MMS Client supports the transport of application specific data.

    Type: Boolean
    Resolution: Locked
    Examples: "Yes", "No"
    Default: "Yes"
   </rdfs:comment>
   <rdfs:range rdf:resource='&prf-dt;Boolean'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>

<rdf:Description rdf:ID="MmsCMFBaseSet">
  <rdf:type rdf:resource="&ns-rdf;Property"/>
  <rdfs:domain rdf:resource="#MmsCharacteristics"/>
  <rdfs:comment xml:lang='en'>
    Description: It indicates that the client support CMF. 
    Legal values are the following pre-defined identifier: "3GPP2-CMF-v1.0" indicates 
    the CMF base set according to 3GPP2 C.S0050-0 v1.0, dated December 12, 2003. 
    Type: Literal bag
    Resolution: Locked
    Examples: "3GPP2-CMF-V1_0"
  </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>


<rdf:Description rdf:ID="MmsDrmClass">
  <rdf:type rdf:resource="&ns-rdf;Property"/>
  <rdfs:domain rdf:resource="#MmsCharacteristics"/>
  <rdfs:comment xml:lang='en'>
	Lists the supported OMA DRM v1.0 download methods.
    Type: Literal bag
    Resolution: Locked
    Examples		“ForwardLock? “CombinedDelivery? ”SeparateDelivery?
  </rdfs:comment>
   <rdfs:range rdf:resource="&ns-rdf;Bag"/>
   <rdfs:range rdf:resource='&prf-dt;Literal'/>
   <prf-base:ResolutionRule rdf:datatype='&prf-dt;ResolutionRule'>Locked</prf-base:ResolutionRule>
</rdf:Description>


</rdf:RDF>
